## AD 2 Aerodromes

### LAKU — KUKES AERODROME

#### LAKU AD 2.1 Aerodrome location indicator and name

LAKU — KUKES Aerodrome

#### LAKU AD 2.2 Aerodrome geographical and administrative data

1 | Aerodrome reference point and its site | 420208N 0202457E Midpoint of RWY 01/19
2 | Direction and distance of aerodrome reference point from centre of the city | 2.82 NM South of Kukes
3 | Aerodrome elevation and reference temperature | 1160 ft/28° C
4 | Geoid undulation at the aerodrome elevation position | 142 ft
5 | Magnetic variation, date of information and annual change | 5°E (2024)/0.1°
6 | Name of aerodrome operator, address, telephone and telefax numbers, e-mail address, AFS address and, if available, website address | Kukes International Airport National Highway Kukës - Peshkopi, Km 3, Shtiqen, Kukës Albania Phone: +355 697015951 E-mail: info@kuiport.al URL: www.kuiport.al
7 | Types of traffic permitted to use the aerodrome (IFR/VFR) | IFR/VFR
8 | Remarks | NIL

#### LAKU AD 2.3 Operational hours

1 | Aerodrome operator | SR - SS
2 | Customs and immigration | H24
3 | Health and sanitation | SR - SS
4 | AIS Briefing Office | NIL
5 | ATS Reporting Office (ARO) | NIL
6 | MET Briefing Office | NIL
7 | ATS | HO
8 | Fuelling | SR - SS
9 | Handling | SR - SS
10 | Security | H24
11 | De-icing | SR - SS
12 | Remarks | All flight operations to and from Kukes Airport are subject to Prior Permission Required (PPR). Operators must submit the application form and the documents to CAA at least three (3) working days in advance prior to the scheduled start of operations. Operators are not allowed to use the airport as an alternate. ATS Reporting Service and MET information are provided by Kukes AFIS unit.

#### LAKU AD 2.4 Handling services and facilities

1 | Cargo-handling facilities | NIL
2 | Fuel and oil types | FUEL: AVGAS - Octane 100 aviation gasoline A1 - Jet A1 aviation fuel By arrangement with fuel company OIL: NIL
3 | Fuelling facilities and capacity | 1 truck 18000 litres
4 | De-icing facilities | Aircraft de-icing fluid, type 1
5 | Hangar space for visiting aircraft | NIL
6 | Repair facilities for visiting aircraft | NIL
7 | Remarks | NIL

#### LAKU AD 2.5 Passenger facilities

1 | Hotels | In the city
2 | Restaurants | In the city
3 | Transportation | Buses, taxis from the AD
4 | Medical facilities | First aid at AD. Hospitals in the city
5 | Bank and Post Office | Bank and Post Office in the city
6 | Tourist Office | Tourist Office in the city
7 | Remarks | NIL

#### LAKU AD 2.6 Rescue and fire fighting services

1 | Aerodrome category for firefighting | Belongs to CAT 6
2 | Rescue equipment | 2 trucks
3 | Capability for removal of disabled aircraft | Push-back tractors and tow bars for MTOW 120 tons
4 | Remarks | NIL

#### LAKU AD 2.7 Seasonal availability - clearing

1 | Seasonal availability | Aerodrome must be used with caution during the winter season of the year.
2 | Type(s) of clearing equipment | Mechanical, chemical de-icing.
3 | Clearance priorities | Runway in use and designated taxiway; Apron; PAPI area if needed; and All other aircraft operating areas not yet cleared.
4 | Use of material for movement area surface treatment | NAAC
5 | Specially prepared winter runways | Not applicable
6 | Remarks | See AD 1.2, subsection 2. for the runway surface condition assessment and reporting.

#### LAKU AD 2.8 Aprons, taxiways and check locations/positions data

1 | Designation, surface and strength of aprons | Designation: MAIN APRON Surface: CONC Strength: PCN 59/R/C/W/T
2 | Designation, width, surface and strength of taxiways | Designation: B Width: 23 M Surface: ASPH Strength: PCN 53/F/A/X/T
3 | Location and elevation of altimeter checkpoints | NIL
4 | Location of VOR checkpoints | NIL
5 | Position of INS checkpoints | NIL
6 | Remarks | NIL

#### LAKU AD 2.9 Surface movement guidance and control system and markings

1 | Use of aircraft stand identification signs, taxiway guide lines and visual docking/parking guidance system at aircraft stands | Approach to the apron is from the taxiway B, following the continuous yellow line markings.Usually aircraft are guided by a “FOLLOW ME” car. The guidance principles are according to the marshaller’s hand signals.
2 | Runway and taxiway markings and lights | RWY 01/19 Markings: Designation numbers and touchdown zoneLGT: Threshold, runway end and runway edges TWY B Markings: Taxi-holding positions and TWY centrelineLGT: Taxiway edges
3 | Stop bars and runway guard lights (if any) | NIL
4 | Other runway protection measures | NIL
5 | Remarks | NIL

#### LAKU AD 2.10 Aerodrome obstacles

##### 1. Obstacles in Area 2

The list of obstacles in Area 2 is available as a digital data set. See GEN 3.1, subsection 6.2.

##### 2. Obstacles in Area 3

The list of obstacles in Area 3 is available as a digital data set. See GEN 3.1, subsection 6.2.

#### LAKU AD 2.11 Meteorological information provided

1 | Name of the associated meteorological office | Kukes MET Office
2 | Hours of service and, where applicable, the designation of the responsible meteorological office outside these hours | HO
3 | Office responsible for preparation of TAFs and periods of validity and interval of issuance of the forecasts | Tirana MET Office Available during operation hours of Kukes AFIS unit (first issued 1 hour prior to the start of operations)
4 | Availability of the trend forecasts for the aerodrome, and interval of issuance | NIL
5 | Information on how briefing and/or consultation is provided | By Kukes AFIS unit (via multimedia)
6 | Types of flight documentation supplied and language(s) used in flight documentation | Aerodrome METAR and TAF EN/AL
7 | Charts and other information displayed or available for briefing or consultation | NIL
8 | Supplementary equipment available for providing information on meteorological conditions, e.g. weather radar andreceiver for satellite images | NIL
9 | The air traffic services unit(s) provided with meteorological information | Kukes AFIS unit
10 | Additional information (e.g. concerning any limitation of service, etc.) | LAKU METAR available during operation hours of Kukes AFIS unit

#### LAKU AD 2.12 Runway physical characteristics

Designation | True bearings | RWY dimensions | RWY/SWY strength (PCN) and surface | THR coordinates RWY end coordinates THR geoid undulation | THR elevation TDZ highest elevation
--- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6
01 | 012.99º | 2198 X 30 M | 50/F/B/X/T/ ASPH | 420128.16N 0202444.35E - 142.3 ft | THR 1160.4 ft -
19 | 192.99º | 2198 X 30 M | 50/F/B/X/T/ ASPH | 420237.60N 0202505.84E - 142.3 ft | THR 1152.2 ft -

Designation | RWY/SWY slope | SWY dimensions | CLR dimensions | Strip dimensions | RESA dimensions
--- | --- | --- | --- | --- | ---
| 7 | 8 | 9 | 10 | 11
01 | - 0.11% | NIL | NIL | 2318 X 150 M | 240 X 150 M
19 | + 0.11% | NIL | NIL | 2318 X 150 M | 90 X 60 M

Designation | Location of arresting system | OFZ | Remarks
--- | --- | --- | ---
| 12 | 13 | 14
01 | NIL | NIL | NIL
19 | NIL | NIL | NIL

#### LAKU AD 2.13 Declared distances

Runway designator | TORA | TODA | ASDA | LDA | Remarks
--- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6
01 | 2198 M | 2198 M | 2198 M | NU | NIL
19 | NU | NU | NU | 2198 M | NIL

#### LAKU AD 2.14 Approach and runway lighting

Runway designator | Approach lighting system type, length and intensity | THR lights colour and wing bars | VASIS type (MEHT) | TDZ lights length
--- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5
01 | NIL | NIL | NIL | NIL
19 | Type: Simple approach lighting system Length: 420 M Intensity: LIH Adjustable in 5 stages | Green | PAPI 3.5° Left (53 ft) | NIL

RWY centre line lights length, spacing, colour and intensity | RWY edge lights length, spacing,colour and intensity | RWY end lights colour and wing bars | Stopway lights length and colour | Remarks
--- | --- | --- | --- | ---
6 | 7 | 8 | 9 | 10
NIL | NIL | NIL | NIL | NIL
NIL | Length: 2 198 M Spacing: 60 M Colour: White Intensity: LIH | Red | NIL | Due to terrain constraints PAPI lights are visible from about 4 km

#### LAKU AD 2.15 Other lighting, secondary power supply

1 | Location, characteristics and hours of operation of aerodrome beacon/identification beacon | ABN: NIL IBN: NIL
2 | Location and lighting of anemometer/landing direction indicator | LDI: NIL Anemometer: NIL
3 | Taxiway edge and taxiway centre line lights | Edge: NIL Centre line: NIL
4 | Secondary power supply/switch-over time | Secondary power supply to all lighting at AD. Switch-over time:12 SEC
5 | Remarks | NIL

#### LAKU AD 2.16 Helicopter landing areas

NIL

#### LAKU AD 2.17 Air traffic service Airspace

Designation and lateral limits | Vertical limits | Class of Airspace | ATS unit call sign/ Language | Transition Altitude | Hours of applicability | Remarks
--- | --- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6 | 7
Kukes FIZ/RMZ 415929N 0203631E - 415901N 0194718E - 422301N 0194651E - 422314N 0201342E along Tirana FIR boundary to the point of origin. | Upper limit: FL115 Lower limit: GND | G | Kukes Aerodrome Information EN | 10000 ft | Applicable during AFIS unit operational hours | Outside AFIS HO, pilots entering Kukes FIZ/RMZ are requested to contact Tirana APP on frequency 133.150 MHz to receive flight information.

#### LAKU AD 2.18 ATS communication facilities

Service Designation | Call sign | Channel(s) | Hours of operation | Remarks
--- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5
AFIS | Kukes Aerodrome Information | 118.375 MHz 119.825 MHz 121.500 MHz Emergency Channel | HO | NIL

#### LAKU AD 2.19 Radio navigation and landing aids

Type of aids MAG Variation VOR/ILS Declination | ID | Frequency/Channel | Hours of operation | Geographical coordinates of transmitting antenna | Elevation of DME transmitting antenna | Remarks
--- | --- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6 | 7
GPS | NIL | 1575.42 MHz | H24 | Tirana FIR | NIL | Operated by US Department of Defense

#### LAKU AD 2.20 Local aerodrome regulations

##### 1. Local regulations

1.1 Local regulations applicable to the traffic at Kukes International Airport are collected in a manual which is available at the Airport Operations Office. This manual includes, among other subjects, the following:

1. the meaning of markings and signs;
2. information about taxiing from aircraft parking positions;
3. limitations in the operation of large aircraft;
4. helicopter operations;
5. marshaller assistance;
6. fuel spillage; and
7. precautions during extreme weather conditions.

1.2 Marshaller assistance can be requested and further information about the regulations can be obtained from the Kukes AFIS unit.
1.3 When a local regulation is of importance for the safe operation of aircraft on the apron, the information will be given to each aircraft by the Kukes AFIS unit.

##### 2. Ground movement

###### 2.1 Parking procedures

2.1.1 Arriving aircraft will be instructed to the main apron by the Kukes AFIS unit. “FOLLOW ME” vehicle will guide the aircraft to the parking stand.
2.1.2 Aircraft landing on Runway 19 are expected to vacate the RWY via TWY B.
2.1.3 General aviation aircraft will be guided by a Marshaller to the apron. Assistance from the “FOLLOW ME” vehicle can be requested via the Kukes AFIS unit.
2.1.4 Since there is no special parking area for helicopters on the aerodrome, helicopters will be instructed by the Kukes AFIS unit to the parking area. Marshaller will guide the helicopter to the parking stand.

###### 2.2 Taxiing

2.2.1 During taxiing, the pilot shall comply with traffic regulation on apron taking into account instructions and information provided by the Kukes AFIS unit in order to avoid collision with other aircraft, vehicles, persons or objects. Neither deviations nor shortcuts are allowed except under the guidance of Marshaller or “FOLLOW ME” vehicle or after special instructions given by the Kukes AFIS unit.
2.2.2 The main apron is used for operation of aircraft category C with maximum wingspan 36 m.

##### 3. CAT II/III operations

Not applicable.

##### 4. School and training flights - technical test flights

4.1 Training and technical flights must only be made after permission has been obtained from the CAA of Albania (see GEN 1.2).
4.2 Application for a training flight shall be submitted at least 10 days in advance of the proposed operation.
4.3 Application for a technical test flight shall be submitted at least 2 hours before such a flight is operated.

##### 5. Removal of disabled aircraft from runway

5.1 When an aircraft is wrecked on a runway, it is the duty of the owner or user of such aircraft to have it removed as soon as possible.
5.2 If a wrecked aircraft is not removed from the runway as quickly as possible by the owner or user, the aircraft will be removed by the aerodrome authority at the owner’s or user’s expense.
5.3 The Aerodrome Coordinator for the removal of disabled aircraft at Kukes International Airport (KFZ) is the Operations Manager, Tel: +355 697015951.

#### LAKU AD 2.21 Noise abatement procedures

No noise abatement procedures are established due to low traffic density.

#### LAKU AD 2.22 Flight procedures

##### 1. General

###### 1.1 Flight Information Zone/Radio Mandatory Zone

1.1.1 A FIZ/RMZ is established around Kukes Airport, applicable during the opening hours of airport.
1.1.2 Flights within the Kukes FIZ/RMZ shall be operated in accordance with the Instrument Flight Rules and Visual Flight Rules.
1.1.3 Flights transiting the Kukes FIZ/RMZ shall establish initial contact with Tirana APP unit before entering the designated area and report:

1. call sign;
2. type of aircraft;
3. position;
4. level; and
5. intentions of the flight.

1.1.4 Flights departing from Kukes Airport shall make position report before requesting taxiing to Kukes AFIS unit.
1.1.5 Flights shall maintain continuous air-ground voice communication watch when present in the Kukes FIZ/RMZ. Flights shall report exiting the Kukes FIZ/RMZ.

###### 1.2 Aerodrome Flight Information Service (AFIS)

1.2.1 Standard FIS and ALS is provided in the Kukes FIZ/RMZ by the Kukes AFIS unit in accordance to SERA Section 9 and Section 10. In particular, the AFIS Officer (AFISO) shall:

- inform IFR flights about any other relevant traffic in the Kukes FIZ/RMZ at all time,
- inform IFR approaches about the availability of the runway and the presence of traffic in the vicinity of the airport, such that the pilots can decide to execute a missed approach due to other traffic when appropriate,
- instruct arriving flights to the apron,
- inform IFR departures about the availability of the runway and the presence of traffic in the vicinity of the airport, such that the pilots can decide to postpone lining up when appropriate,
- transmit ATC departure clearance as provided by Tirana APP Unit for IFR/VFR traffic which plan to cross controlled airspace,
- pass instructions to vehicles and personnel operating on the maneuvering area,
- inform all relevant VFR flights about IFR flights in the Kukes FIZ/RMZ.

1.2.2 AFISO shall provide information to departing and arriving aircraft that the runway is free when no aircraft, vehicles or other obstructions are on the runway or safety strip.

##### 2. Procedures for IFR flights within Kukes FIZ/RMZ

###### 2.1 General remarks

2.1.1 The procedures differ partly from standard ICAO procedures as described in GEN 1.7.
2.1.2 Due to the mountainous terrain in the vicinity of the aerodrome and the requirement for visual manoeuvring, it is considered essential that pilots are well familiar with descent, approach and missed approach procedures, balked landing procedures as well as the visual manoeuvres, and the departure procedures. The responsibility for the preparation of such information rests with the operator for commercial flights, respectively pilot in command (for non-commercial flights).

###### 2.2 Information on design and other details

2.2.1 The design of any departure contingency procedure and balked landing procedure during the visual approach procedure is the responsibility of the operator / pilot in command. These procedures need to be tailored for the specific aircraft types and their performance.

###### 2.3 Aerodrome examination

2.3.1 Site examination by captains or training with a flight simulator equipped with an approved specific external vision system is recommended.

###### 2.4 Special instructions

2.4.1 No take-offs and landings at night.
2.4.2 One engine out approaches should not be executed except in case of emergency justifying opposite decision.
2.4.3 Kukes FIZ/RMZ is a Class G airspace in which AFIS is provided, and due to maneuvering area layout, Tirana APP, in coordination with Kukes AFIS unit, will ensure that only one aircraft at a time will land or take-off.
2.4.4 In this respect, Tirana APP will decide the release time for IFR departures from LAKU in order not to interfere with the flight path of arriving IFR aircraft.

###### 2.5 Arrivals

2.5.1 STARs are published as RNAV1 based on GNSS. Aircraft will follow the appropriate STAR to the Initial Approach Fix (IAF) for the RNP RWY19 approach as instructed by Tirana APP.

###### 2.6 Holding

2.6.1 There is a holding facility located at the IAF SINNE, inbound TR075° right turns, outbound TR255°, 1 minute, minimum holding altitude 10000 ft. After passing SINNE, the aircraft proceeding on the initial approach for the RNP RWY19 procedure shall contact Pristina APP on frequency 135.475 MHz or 125.980 MHz.

###### 2.7 Approach

2.7.1 An RNP approach procedure is in use for RWY19 only. The nominal track is based on a 3.5° glide slope from KU503 (FAF) to touchdown. When established on the final approach, the pilot shall descend using a CDFA approach technique after passing the FAF. After KU504 (MAPt) the procedure is continued as a visual approach procedure.
2.7.2 Visual reference to terrain with minimum visibility 5 KM and ceiling 2300 ft AAL or above is required not later than KU504, prior to continuing with the visual segment of the procedure. For category A aircraft a ceiling of 1200 ft AAL is required to perform a visual circuit in case of a go-around.

###### 2.8 Missed approach

2.8.1 At the MAPt (KU504), turn right to KU505, while climbing to 10000 ft AMSL, then continue to SINNE and join holding. Note the required climb gradient of 4%.
2.8.2 If unable to comply with minimum holding altitude, turn right at SINNE to establish on initial approach track of RNP procedure and continue climb to MSA. After passing the MSA altitude, continue climb to FL120 and turn right to join holding pattern at SINNE.
2.8.3 In case of initiating a missed approach before the MAPt, continue the final approach track until reaching the MAPt before making the right turn.

###### 2.9 Landing

2.9.1 Landings RWY19 only. PAPI is required for RWY19.
2.9.2 Circling RWY01 not allowed.
2.9.3 Special attention must be paid to the visual manoeuvring during the final phase of approach. The alignment with the runway centreline requires precise manoeuvring. The 3.5° descent path and non-standard width runway may create an illusion of being too high. That increases the probability of a balked landing, which is difficult to execute due to the high terrain surrounding the airport.
2.9.4 In case of a go-around, initiate climb and proceed with right turn no later than at the end of the runway at a safe altitude. Proceed visually to KU505, keeping separation to terrain. Note that TAWS alerts may occur during visual manoeuvring. At KU505 join the published missed approach procedure for the RNP RWY19 approach.
2.9.5 Optionally, category A aircraft only, join a right hand downwind for a second landing attempt on RWY19. Minimum visibility 5 KM and ceiling 1200 ft AAL or above is required.

###### 2.10 Take-off

2.10.1 Take-off RWY01 only. Apply NADP1 noise abatement procedure until passing 3000 ft AAL. Strictly adhere to SID procedure.
2.10.2 Turning before the DER may result in undesired proximity to obstacles.
2.10.3 Note the Standard Instrument Departure minimum climb gradients of 9.5% until passing 5000 ft AMSL and 4.3% until passing FL120.

###### 2.11 Radio communication failure procedures

2.11.1 In the event of complete radio communication failure in an aircraft, the pilot is to adopt the procedures described at GEN 3.3.

##### 3. Procedures for VFR flights within Kukes FIZ/RMZ

###### 3.1 General

3.1.1 VFR flights shall comply with the provisions of SERA Section 4 and Section 5 when operated within or into the Kukes FIZ/RMZ.
3.1.2 An aircraft conducting VFR flight shall enter, transit or exit Kukes FIZ/RMZ via the VFR reporting points depicted on the Visual Approach Chart - ICAO at LAKU AD 2.24-13 unless otherwise authorised by ATC.
3.1.3 A flight plan is required for VFR operations in the Kukes FIZ/RMZ. Procedures relating to VFR flight plan are detailed at ENR 1.10.
3.1.4 Local VFR traffic in the Kukes FIZ/RMZ should avoid flying near the IFR flight paths and should adhere strictly to the requirements for continuous two-way radio communication and reporting of position and flight level.
3.1.5 VFR reporting points are as follows:

Name | Location | Coordinates
KUKES | Qafë Morinë (Morina Pass) | 421003N 0203233E
JAKOV* | Mali i Pëllumit (Pëllumi Mountain) | 422208N 0201441E
DRINO | Liqeni i Vaut të Dejës (Vau i Dejës Lake) | 420435N 0194712E
TUNEL | Tuneli i Kalimashit (Kalimash Tunnel) | 415918N 0201230E

*JAKOV point for military NATO/KFOR flights only.

3.1.6 All VFR reporting points are compulsory reporting points .

###### 3.2 Landing

3.2.1 Pilots shall use the standard right-hand traffic pattern when arriving at the airport.
3.2.2 The traffic pattern altitude should be maintained until the aircraft is at least abeam the approach end of the landing runway on the downwind leg. The base leg turn should commence when the aircraft is at a point approximately 45 degrees relative bearing from the approach end of the runway.
3.2.3 Helicopters operating in the traffic pattern when landing on the runway may fly a pattern similar to the fixed-wing aircraft traffic pattern but at a lower altitude (500 feet AGL) and closer to the runway.
3.2.4 Landing should be accomplished on the operating Runway 19 most nearly aligned into the wind.
3.2.5 Airplanes should not be operated in the traffic pattern at an indicated airspeed of more than 200 knots.

###### 3.3 Take-off

3.3.1 Airplanes on take-off should continue straight ahead until beyond the departure end of the Runway 01.

###### 3.4 Radio communications failure procedures

3.4.1 In the event of complete radio communications failure in a VFR flight, the pilot is to adopt the procedures detailed at GEN 3.3.

#### LAKU AD 2.23 Additional Information

##### 1. Bird control and animal hazard

1.1 The warning regarding the presence of bird and animal hazards can be passed to aircraft via Kukes AFIS unit.
1.2 Kukes Airport Operations will carry out bird patrols on a continuous basis throughout the day with specific inspection on the runways and strips.
1.3 In the event of a prolonged problem with birds on or in the vicinity of the airport, details will be promulgated by NOTAM. This will only cover periods of short or medium duration and will be cancelled when the hazard ceases to exist.

#### LAKU AD 2.24 Charts related to the aerodrome

Name | Page
Aerodrome Chart (ADC) - ICAO
../graphics/eAIP/ADC2024102911015103660000.pdf
Aerodrome Obstacle Chart (AOC) - ICAO Type A RWY 01
../graphics/eAIP/ADC2024102908182707920000.pdf
Standard Departure Chart - Instrument (SID) - ICAO RNAV RWY 01
../graphics/eAIP/ADC2024051709205700770000.pdf
Standard Arrival Chart - Instrument (STAR) - ICAO RNAV RWY 19
../graphics/eAIP/ADC2024051709222508440000.pdf
Instrument Approach Chart (IAC) - ICAO RNP (LNAV only) RWY 19
../graphics/eAIP/ADC2024051709234905340000.pdf
Visual Approach Procedure Chart – RWY 19
../graphics/eAIP/ADC2024051709244705370000.pdf
Visual Approach Chart (VAC) – ICAO
../graphics/eAIP/ADC2024102509025100570000.pdf

#### LAKU AD 2.25 Visual Segment Surface (VSS) penetration

Not applicable