### GEN 2.4 Location indicators

The location indicators marked with an asterisk (*) can not be used in the address component of the AFTN messages.

1. ENCODE
Location | Indicator
GJADER MIL. AIRPORT | LAGJ*
KORCA AIRFIELD | LAKO*
KUCOVA MIL. AIRPORT | LAKV*
KUKES AERODROME | LAKU
SARANDA AIRFIELD | LASR*
SHKODER AIRFIELD | LASK*
TIRANA AERODROME | LATI
TIRANA AFTN COM CENTRE | LAAA
TIRANA FIR/ACC/FIC/SAR | LAAA
TIRANA MIL. HELIPORT | LAFK*
TIRANA NOF | LAAA
VLORA AIRFIELD | LAVL*
2. DECODE
Indicator | Location
LAAA | TIRANA FIR/ACC/FIC/SAR
LAAA | TIRANA AFTN COM CENTRE
LAAA | TIRANA NOF
LAFK* | TIRANA MIL. HELIPORT
LAGJ* | GJADER MIL. AIRPORT
LAKO* | KORCA AIRFIELD
LAKU | KUKES AERODROME
LAKV* | KUCOVA MIL. AIRPORT
LASK* | SHKODER AIRFIELD
LASR* | SARANDA AIRFIELD
LATI | TIRANA AERODROME
LAVL* | VLORA AIRFIELD