## ENR 3 ATS Routes

### ENR 3.2 Area navigation routes

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (2) Navigation accuracy requirement: ±5 NM (3) For continuation see AIP Serbia & Montenegro
L187 |
▲ | TIRCA | 403304N 0195123E TRN 168° 52.2 NM (100 FT) |  |
(RNAV 5) |
323
-
| 64.4 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2)
▲ | RODON (FIR BDRY) | 412730N 0190600E TRN 270° 28.0 NM (100 FT) |  | (3)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (13) Navigation accuracy requirement: ±5 NM (14) For continuation see AIP Greece (15) For continuation see AIP Serbia & Montenegro
L604 |
▲ | DIMIS (FIR BDRY) | 400421N 0203541E TRN 148° 90.0 NM (100 FT) |  | (14)
(RNAV 5) |
329
149
| 30.2 NM |
FL 195
FL 115
| Even(1) | Odd(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (13)
∆ | ADDER | 403126N 0201817E TRN 148° 59.8 NM (100 FT) |  |
(RNAV 5) |
329
148
| 22.8 NM |
FL 195
FL 115
| Even(3) | Odd(4) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (3) H24 (4) H24 (13)
▲ | ELBAK | 405151N 0200452E TRN 148° 37.0 NM (100 FT) |  |
(RNAV 5) |
329
149
| 13.7 NM |
FL 195
FL 115
| Even(5) | Odd(6) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (5) H24 (6) H24 (13)
∆ | UNDER | 410405N 0195651E TRN 149° 23.3 NM (100 FT) |  |
(RNAV 5) |
329
149
| 23.3 NM |
FL 195
FL 115
| Even(7) | Odd(8) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (7) H24 (8) H24 (13)
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |
(RNAV 5) |
336
156
| 35.9 NM |
FL 195
FL 115
| Even(9) | Odd(10) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (9) H24 (10) H24 (13)
▲ | INLOT | 415847N 0192711E TRN 336° 35.8 NM (100 FT) |  |
(RNAV 5) |
336
156
| 15.8 NM |
FL 195
FL 115
| Even(11) | Odd(12) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (11) H24 (12) H24 (13)
▲ | RETRA (FIR BDRY) | 421342N 0192006E POD 154.3° 10.1 NM (158 FT) |  | (15)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (2) Navigation accuracy requirement: ±5 NM (3) For continuation see AIP Serbia & Montenegro
L607 |
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |
(RNAV 5) |
-
135
| 28.2 NM |
FL 195
FL 115
|  | Odd(1) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2)
▲ | PETAK (FIR BDRY) | 414631N 0191850E POD 170.8° 36.7 NM (158 FT) |  | (3)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP Greece (5) For continuation see AIP Serbia & Montenegro
L611 |
▲ | TUMBO (FIR BDRY) | 400402N 0202822E TRN 152° 87.9 NM (100 FT) |  | (4)
(RNAV 5) |
319
-
| 35.5 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (3)
∆ | OVVER | 403230N 0200046E TRN 161° 54.1 NM (100 FT) |  |
(RNAV 5) |
318
-
| 68.9 NM |
FL 195
FL 115
| Even(2) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (2) H24 (3)
▲ | RODON (FIR BDRY) | 412730N 0190600E TRN 270° 28.0 NM (100 FT) |  | (5)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (5) Navigation accuracy requirement: ±5 NM (6) For continuation see AIP Italy
M26 |
▲ | GOKEL (FIR BDRY) | 403554N 0190000E TRN 209° 58.9 NM (100 FT) |  | (6)
(RNAV 5) |
028
209
| 25.0 NM |
FL 195
FL 115
| Odd(1) | Even(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (5)
▲ | DITAN | 405644N 0191813E TRN 209° 33.9 NM (100 FT) |  |
(RNAV 5) |
028
209
| 33.9 NM |
FL 195
FL 115
| Odd(3) | Even(4) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (3) H24 (4) H24 (5)
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (7) Navigation accuracy requirement: ±5 NM (8) For continuation see AIP Greece (9) For continuation see AIP Serbia & Montenegro
M127 |
▲ | NIKRO (FIR BDRY) | 393957N 0200712E TRN 165° 106.5 NM (100 FT) |  | (8)
(RNAV 5) |
350
-
| 52.8 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (7)
∆ | OVVER | 403230N 0200046E TRN 161° 54.1 NM (100 FT) |  |
(RNAV 5) |
341
-
| 54.2 NM |
FL 195
FL 115
| Even(2) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (2) H24 (7)
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |
(RNAV 5) |
000
180
| 34.2 NM |
FL 195
FL 115
| Odd(3) | Even(4) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (3) H24 (4) H24 (7)
▲ | RINAV | 415901N 0194718E TRN 000° 34.2 NM (100 FT) |  |
(RNAV 5) |
000
180
| 29.9 NM |
FL 195
FL 115
| Odd(5) | Even(6) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (5) H24 (6) H24 (7)
▲ | ALELU (FIR BDRY) | 422845N 0195102E TRN 000° 64.0 NM (100 FT) |  | (9)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (11) Navigation accuracy requirement: ±5 NM (12) For continuation see AIP Italy (13) For continuation see AIP Greece
M603 |
▲ | GOKEL (FIR BDRY) | 403554N 0190000E TRN 209° 58.9 NM (100 FT) |  | (12)
(RNAV 5) |
089
269
| 24.2 NM |
FL 195
FL 115
| Odd(1) | Even(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (11)
▲ | LIMJA | 403412N 0193145E TRN 185° 51.5 NM (100 FT) |  |
(RNAV 5) |
089
270
| 15.0 NM |
FL 195
FL 115
| Odd(3) | Even(4) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (3) H24 (4) H24 (11)
▲ | TIRCA | 403304N 0195123E TRN 168° 52.2 NM (100 FT) |  |
(RNAV 5) |
090
270
| 7.2 NM |
FL 195
FL 115
| Odd(5) | Even(6) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (5) H24 (6) H24 (11)
∆ | OVVER | 403230N 0200046E TRN 161° 54.1 NM (100 FT) |  |
(RNAV 5) |
090
270
| 13.4 NM |
FL 195
FL 115
| Odd(7) | Even(8) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (7) H24 (8) H24 (11)
∆ | ADDER | 403126N 0201817E TRN 148° 59.8 NM (100 FT) |  |
(RNAV 5) |
090
270
| 29.9 NM |
FL 195
FL 115
| Odd(9) | Even(10) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (9) H24 (10) H24 (11)
▲ | PINDO (FIR BDRY) | 402851N 0205721E TRN 130° 79.4 NM (100 FT) |  | (13)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (2) Navigation accuracy requirement: ±5 NM (3) For continuation see AIP North Macedonia
N141 |
▲ | DOBAR (FIR BDRY) | 411958N 0202941E TRN 093° 35.4 NM (100 FT) |  | (3)
(RNAV 5) |
-
093
| 35.4 NM |
FL 195
FL 115
|  | Odd(1) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2)
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP Greece (5) For continuation see AIP Serbia & Montenegro
N732 |
▲ | PITAS (FIR BDRY) | 395400N 0195040E TRN 171° 91.1 NM (100 FT) |  | (4)
(RNAV 5) |
-
155
| 42.8 NM |
FL 195
FL 115
|  | Odd(1) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (3)
▲ | LIMJA | 403412N 0193145E TRN 185° 51.5 NM (100 FT) |  |
(RNAV 5) |
-
155
| 56.8 NM |
FL 195
FL 115
|  | Odd(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (2) H24 (3)
▲ | RODON (FIR BDRY) | 412730N 0190600E TRN 270° 28.0 NM (100 FT) |  | (5)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (9) Navigation accuracy requirement: ±5 NM (10) For continuation see AIP Italy (11) For continuation see AIP North Macedonia
P92 |
▲ | PAPIZ (FIR BDRY) | 405330N 0185706E TRN 223° 46.9 NM (100 FT) |  | (10)
(RNAV 5) |
043
223
| 14.8 NM |
FL 195
FL 115
| Odd(1) | Even(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (9)
▲ | DIRES | 410328N 0191133E TRN 223° 32.1 NM (100 FT) |  |
(RNAV 5) |
043
223
| 32.1 NM |
FL 195
FL 115
| Odd(3) | Even(4) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (3) H24 (4) H24 (9)
▲ | TIRANA DVOR/DME (TRN) | 412458N 0194306E |  |
(RNAV 5) |
062
242
| 22.3 NM |
FL 195
FL 115
| Odd(5) | Even(6) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (5) H24 (6) H24 (9)
▲ | ODRAS | 413335N 0201027E TRN 062° 22.3 NM (100 FT) |  |
(RNAV 5) |
062
243
| 17.3 NM |
FL 195
FL 115
| Odd(7) | Even(8) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (7) H24 (8) H24 (9)
▲ | MAVAR (FIR BDRY) | 414012N 0203148E TRN 062° 39.6 NM (100 FT) |  | (11)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (2) Navigation accuracy requirement: ±5 NM (3) For continuation see AIP Serbia & Montenegro
T2 |
▲ | DIRES | 410328N 0191133E TRN 223° 32.1 NM (100 FT) |  |
(RNAV 5) |
298
-
| 15.2 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2)
▲ | EBELA (FIR BDRY) | 411136N 0185432E |  | (3)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP Greece
T6 |
▲ | PINDO (FIR BDRY) | 402851N 0205721E TRN 130° 79.4 NM (100 FT) |  | (4)
(RNAV 5) |
295
-
| 22.1 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (3)
∆ | NURSO | 403956N 0203217E TRN 135° 58.4 NM (100 FT) |  |
(RNAV 5) |
295
-
| 24.0 NM |
FL 195
FL 115
| Even(2) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (2) H24 (3)
▲ | ELBAK | 405151N 0200452E TRN 148° 37.0 NM (100 FT) |  |

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (2) Navigation accuracy requirement: ±5 NM (3) For continuation see AIP Serbia & Montenegro
T8 |
▲ | INLOT | 415847N 0192711E TRN 336° 35.8 NM (100 FT) |  |
(RNAV 5) |
-
186
| 34.0 NM |
FL 195
FL 115
|  | Even(1) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2)
▲ | AKIKA (FIR BDRY) | 423203N 0193614E POD 055.1° 17.9 NM (158 FT) |  | (3)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP North Macedonia
T216 |
▲ | ODRAS | 413335N 0201027E TRN 062° 22.3 NM (100 FT) |  |
(RNAV 5) |
128
309
| 19.9 NM |
FL 195
FL 115
| Odd(1) | Even(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (3)
▲ | DOBAR (FIR BDRY) | 411958N 0202941E TRN 093° 35.4 NM (100 FT) |  | (4)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP Greece (5) For continuation see AIP Serbia & Montenegro
Y132 |
▲ | NIKRO (FIR BDRY) | 393957N 0200712E TRN 165° 106.5 NM (100 FT) |  | (4)
(RNAV 5) |
342
-
| 54.5 NM |
FL 195
FL 115
| Even(1) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (3)
▲ | TIRCA | 403304N 0195123E TRN 168° 52.2 NM (100 FT) |  |
(RNAV 5) |
342
-
| 103.5 NM |
FL 195
FL 115
| Even(2) |  | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (2) H24 (3)
▲ | RETRA (FIR BDRY) | 421342N 0192006E POD 154.3° 10.1 NM (158 FT) |  | (5)

Route designator | Route Remarks (Optional) |
--- | --- | ---
| Names, coded designators or name-codes | Significant point geographical coordinates Reference VOR/DME ID Bearing and distance DME Elevation |  |  | Significant Point Remarks
Navigation accuracy requirement {RNAV / RNP Type} | MAG bearing ↓ / ↑ | Geodesic distance |
Upper limit
Lower limit
| Direction of cruising levels | Remarks Controlling unit, Operating channel, and logon address {Airspace Classification} Navigation specification(s) limitations
↓ | ↑
Point/Segment Remarks: (3) Navigation accuracy requirement: ±5 NM (4) For continuation see AIP North Macedonia (5) For continuation see AIP Serbia & Montenegro
Y400 |
▲ | MAVAR (FIR BDRY) | 414012N 0203148E TRN 062° 39.6 NM (100 FT) |  | (4)
(RNAV 5) |
298
117
| 63.1 NM |
FL 195
FL 115
| Even(1) | Odd(2) | Tirana ACC 127.500 MHz Tirana APP 133.150 MHz {C} (1) H24 (2) H24 (3)
▲ | RETRA (FIR BDRY) | 421342N 0192006E POD 154.3° 10.1 NM (158 FT) |  | (5)